1. Please look at the LAB03\_Architecture Diagram
2. To perform MUL, I assign 4’b1000 as the control\_input to ALU
3. My lab02 architecture using 3x1 multiplexer to do zero extension, if needed please check my LAB02 architecture on my LAB02 report

Last Edited: SAT 11/16